

**SKN\_N0484\_R1**

History and List of changes for SK SRs **SKN\_N0444**

# History, List of changes for SKN\_N0444

**SKN\_N0444\_R1.**

**SKN\_N0444\_R1 approved on 2019-03-07**

- 2019-03-07 "Annex G" approved in M26 and integrated in the SRs

- 2019-03-07 "Annex D" approved in M26 and integrated in the SRs. Content which is in EN 12976:2017 was removed from the SK SR

- 2019-03-07 "Annex O" approved in M26 and added as Annex P5.5 in the SRs

- 2019-04-15 ‘Annex P1\_R2” approved by correspondence and included in SK SRs

- 2019-05-15 Approved by correspondence the inclusion of «aperture area” of the collector in Scenocalc Datasheet

- 2019-05-15 Approved by correspondence the addition of the ηa to the Scenocalc Datasheet on the proposed way according to “SKN\_N0469R0”

**SKN\_N0444\_R2**

**-** **SKN\_N0444\_R2 approved on 2019-11-25**

- 2019-11-25 M27.R1 for “Remote factory inspection” approved in M27 and included in SK SR, in §7.2, as follows:

"The method of remote factory inspection is applicable for interim and follow up inspections under the following conditions:

* Within the period of validity of a certificate (5 years), maximum two remote inspections might be performed.
* Two serial remote inspections are not allowed.
* The use of the method remote inspection *as well as the performing inspector has to be confirmed by the CB individually and in advance.*
* *If former inspections had shown serious non conformities, the CB should deny the use of remote inspection method.*
* *Initial inspections are excluded from remote inspection method.*
* *This method is preliminary accepted for two years and will be evaluated in autumn meeting 2021 after discussion of gained experiences*."

*-* 2019-11-25 M27.R2 for “*Annex 5.6” approved in M27 and added in SK SR*

- 2019-11-25 M27.R3 for “*Annex P5.1 PVT\_R1” approved in M27 and added in SK SR*